### noDataGaps

This processor checks the data returned from the dataCenter for gaps larger than the sample period of the instrument. If from the begin time of the earliest piece to the end time of the latest piece there are no gaps in time larger than the sample period, this process passes the data onto the next item in the line.

### Example

    <noDataGaps/>

### This consists of

<noDataGaps/>

### Places this can be found

In seismogramProcess there is a choice between all of the following

- printlineSeismogramProcess
- sacWriter
- mseedWriter
- asciiWriter
- wavWriter
- recordSectionDisplayGenerator
- responseGain
- phaseCut
- requestCut
- merge
- gapFill
- rMean
- rTrend
- taper
- externalWaveformProcess
- seismogramScript
- localSeismogramTemplateGenerator
- filter
- rms
- oregonDSPFilter
- forkProcess
- alwaysSuccess
- phaseSignalToNoise
- compoundPhaseSignalToNoise
- seismogramImageProcess
- legacyExecute
- seismogramAND
- seismogramOR
- seismogramNOT
- someDataCoverage
- noDataGaps
- fullDataCoverage
- integrate
- differentiate
- transferResponse
- collapseOverlaps
- div
- mul
- invertFlippedChannels
- seismogramSampling
- decimate
- stddev
- rms
- mean
- minMax
- compressionType
- availableDataPlus