### stationHas

The output is true if at least one channel in the station matches each of the enclosed channel subsetters. For example this could be used with a channelNOT to select SH? only if the station does not have BH?.

### Example

    <stationHas>
      <siteCode>00</siteCode>
    </stationHas>

### This consists of

<stationHas>

channel At least once choice
<alwaysSuccess>
<bandCode>
<channelAND>
<channelCode>
<channelEffectiveTimeOverlap>
<channelNOT>
<channelOR>
<channelScript>
<clockId>
<clockManufacturer>
<clockModel>
<clockSerial>
<clockType>
<dasId>
<dasManufacturer>
<dasModel>
<dasSerial>
<dasStyle>
<externalChannelSubsetter>
<gainCode>
<hadDataLastWeek>
<hasNegativeSensitivity/>
<hasResponse/>
<hasSensitivity/>
<isFlipped/>
<isGroupable/>
<orientationAzimuthRange>
<orientationCode>
<orientationDipRange>
<orientationRange>
<printlineChannelProcess>
<repairSensitivity/>
<responseFilterType>
<responseWriter>
<sacPoleZeroWriter>
<sampling>
<sensorId>
<sensorManufacturer>
<sensorModel>
<sensorNominalHighFreq>
<sensorNominalLowFreq>
<sensorSerial>
<siteArea>
<siteBoxArea>
<siteCode>
<siteDepthRange>
<siteEffectiveTimeOverlap>
<sitePolygonFile>
<stageInputUnit>
<stageOutputUnit>
<stageTransferType>
<stationHas>
</stationHas>

### Places this can be found

In channel there is a choice between all of the following

- siteCode
- siteDepthRange
- siteEffectiveTimeOverlap
- siteArea
- siteBoxArea
- sitePolygonFile
- channelCode
- bandCode
- gainCode
- orientationCode
- sampling
- channelEffectiveTimeOverlap
- orientationRange
- orientationAzimuthRange
- orientationDipRange
- channelAND
- channelOR
- channelNOT
- externalChannelSubsetter
- hadDataLastWeek
- printlineChannelProcess
- responseWriter
- sacPoleZeroWriter
- stationHas
- alwaysSuccess
- hasResponse
- hasSensitivity
- repairSensitivity
- responseFilterType
- stageTransferType
- stageInputUnit
- stageOutputUnit
- clockId
- clockManufacturer
- clockModel
- clockSerial
- clockType
- dasId
- dasManufacturer
- dasModel
- dasSerial
- dasStyle
- sensorId
- sensorManufacturer
- sensorModel
- sensorSerial
- sensorNominalHighFreq
- sensorNominalLowFreq
- hasNegativeSensitivity
- isFlipped
- isGroupable
- channelScript