### stationBoxArea

Accepts stations that occur within the latitude longitude box defined here

### Example

    <stationBoxArea>
      <latitudeRange>
        <min>35</min>
        <max>35</max>
      </latitudeRange>
      <longitudeRange>
        <min>-80</min>
        <max>-80</max>
      </longitudeRange>
    </stationBoxArea>

### This consists of

<stationBoxArea>

<latitudeRange>
<longitudeRange>
</stationBoxArea>

### Places this can be found

fdsnStation contains this directly

In station there is a choice between all of the following

- stationCode
- stationRegularExpression
- stationName
- stationOperator
- stationDepthRange
- stationEffectiveTimeOverlap
- stationArea
- stationBoxArea
- stationPolygonFile
- stationPointDistance
- stationPointAzimuth
- printlineStationProcess
- stationPointBackAzimuth
- stationAND
- stationOR
- stationNOT
- externalStationSubsetter
- belongsToVirtual
- stationScript