### stationPointAzimuth

True if the station is within the given azimuth range of the given lat and lon. In keeping with common seismic terminology, azimuth is measured from the point to the station.

### Example

    <stationPointAzimuth>
      <latitude>35</latitude>
      <longitude>-80</longitude>
      <unit>KILOMETER</unit>
      <min>0</min>
      <max>36</max>
    </stationPointAzimuth>

### This consists of

<stationPointAzimuth>

latLonUnitRange interleave
<latitude>
<longitude>
range
</stationPointAzimuth>

### Places this can be found

In station there is a choice between all of the following

- stationCode
- stationRegularExpression
- stationName
- stationOperator
- stationDepthRange
- stationEffectiveTimeOverlap
- stationArea
- stationBoxArea
- stationPolygonFile
- stationPointDistance
- stationPointAzimuth
- printlineStationProcess
- stationPointBackAzimuth
- stationAND
- stationOR
- stationNOT
- externalStationSubsetter
- belongsToVirtual
- stationScript