### alwaysSuccess

Allows a failing channel subsetter to run while passing the channel onto the waveform arm. This can be useful if you only want to run a particular processor if a channel meets a certain criteria, but you want the waveform arm to process it regardless.

### Example

    <alwaysSuccess/>

### This consists of

<alwaysSuccess>

channelPlus Any number of times choice
channel
stationPlus
</alwaysSuccess>

### Places this can be found

In channel there is a choice between all of the following

- siteCode
- siteDepthRange
- siteEffectiveTimeOverlap
- siteArea
- siteBoxArea
- sitePolygonFile
- channelCode
- bandCode
- gainCode
- orientationCode
- sampling
- channelEffectiveTimeOverlap
- orientationRange
- orientationAzimuthRange
- orientationDipRange
- channelAND
- channelOR
- channelNOT
- externalChannelSubsetter
- hadDataLastWeek
- printlineChannelProcess
- responseWriter
- sacPoleZeroWriter
- stationHas
- alwaysSuccess
- hasResponse
- hasSensitivity
- repairSensitivity
- responseFilterType
- stageTransferType
- stageInputUnit
- stageOutputUnit
- clockId
- clockManufacturer
- clockModel
- clockSerial
- clockType
- dasId
- dasManufacturer
- dasModel
- dasSerial
- dasStyle
- sensorId
- sensorManufacturer
- sensorModel
- sensorSerial
- sensorNominalHighFreq
- sensorNominalLowFreq
- hasNegativeSensitivity
- isFlipped
- isGroupable
- channelScript