### availableDataAND

The output is the logical AND of the outputs of all included AvailableData subsetters. This means that it will evaluate to true only if all the enclosed AvailableData subsetters evaluate to true. The subsetters after the first false outputted are not evaluated.

### Example

    <availableDataAND>
        <noGaps />
        <fullCoverage />
    </availableDataAND>

### This consists of

<availableDataAND>

availableDataPlus At least once choice
availableData
channel
eventChannel
eventStation
origin
request
</availableDataAND>

### Places this can be found

In availableData there is a choice between all of the following

- fullCoverage
- postEventWait
- noGaps
- someCoverage
- subrequestCoverage
- percentCoverage
- availableDataAND
- availableDataOR
- availableDataNOT
- availableDataScript
- externalAvailableDataSubsetter
- printlineAvailableDataProcess