### siteDepthRange

Matches sites at a range of depths below the surface. This might be used to separate surface sites from borehole sites.

### Example

    <siteDepthRange>
        <unit>METER</unit>
        <min>100</min>
        <max>200</max>
    </siteDepthRange>

### This consists of

<siteDepthRange>

<unit>
<min>double</min> optional
<max>double</max> optional
</siteDepthRange>

### Places this can be found

In channel there is a choice between all of the following

- siteCode
- siteDepthRange
- siteEffectiveTimeOverlap
- siteArea
- siteBoxArea
- sitePolygonFile
- channelCode
- bandCode
- gainCode
- orientationCode
- sampling
- channelEffectiveTimeOverlap
- orientationRange
- orientationAzimuthRange
- orientationDipRange
- channelAND
- channelOR
- channelNOT
- externalChannelSubsetter
- hadDataLastWeek
- printlineChannelProcess
- responseWriter
- sacPoleZeroWriter
- stationHas
- alwaysSuccess
- hasResponse
- hasSensitivity
- repairSensitivity
- responseFilterType
- stageTransferType
- stageInputUnit
- stageOutputUnit
- clockId
- clockManufacturer
- clockModel
- clockSerial
- clockType
- dasId
- dasManufacturer
- dasModel
- dasSerial
- dasStyle
- sensorId
- sensorManufacturer
- sensorModel
- sensorSerial
- sensorNominalHighFreq
- sensorNominalLowFreq
- hasNegativeSensitivity
- isFlipped
- isGroupable
- channelScript