### find_stations

find_stations produces a recipe containing a networkArm.

### Options

-v/--version | Print SOD's version and exit |
-r/--recipe | Print the created recipe to stdout instead of running it |
-h/--help | Print a brief help message and exit |
-p/--props <props> | Add an additional props file to specify a different nameserver, database or other internal SOD options |
-S/--server <server> | Set the network server to use for this search | sevice.iris.edu
-R/--box-area <box> | Limit the stations to those in a box region. It's specified as west/east/south/north where west and east are longitudes from -180 to 180 and north and south are latitudes from -90 to 90 |
-d/--donut <donut> | Limits the stations to those in a donut region. It's specified as centerLat/centerLon/minRadiusDegrees/maxRadiusDegrees. As with --box-area, latitude goes from -90 to 90 and longitude goes from -180 to 180 |
-s/--stations s1,s2,...,sN | The codes of stations to retrieve like `ANMO` or `KONO`. If unspecified, all stations for retrieved networks will be retrieved |
-n/--networks n1,n2,...,nN | The codes of networks to retrieve like `IU` or `GT`. If unspecified, all networks will be retrieved |
-o/--output <output> | The format for output. Can be none, xy, yx or a Velocity template as described in the printline ingredient | xy