### linearDistanceMagnitudeRange

If the magnitude of the event is greater than or equal to the linear interpolation at the event station distance, then the event station pair is accepted. To reverse and take events smaller than the linear interpolation, enclose this in an EventStationNOT.

### Example

    <linearDistanceMagnitudeRange>
        <magnitudeRange>
            <magType>mb</magType>
            <magType>M</magType>
            <min>5.5</min>
        </magnitudeRange>
        <unit>DEGREE</unit>
        <min>30</min>
        <max>90</max>
    </linearDistanceMagnitudeRange>

### This consists of

<linearDistanceMagnitudeRange>

<magnitudeRange>
range
</linearDistanceMagnitudeRange>

### Places this can be found

In eventStation there is a choice between all of the following

- distanceRange
- printlineEventStation
- azimuthRange
- backAzimuthRange
- linearDistanceMagnitudeRange
- eventStationAND
- eventStationOR
- eventStationNOT
- midPoint
- removeStationDuplicate
- phaseExists
- phaseWithoutInterference
- eventStationScript
- externalEventStationSubsetter