### printlineEventStation

This simply prints a line to standard out or a file for each event-station pair to be processed. It can be used as a simple status monitor. Both filename and template are Velocity templates. They contain site, station, net and event variables. If no template element is given, it defaults to "Got $seismograms.size() seismograms for $channel.codes for eq on $event.time". If no filename is given, the output goes to standard out.

### Example

    <printlineEventStation/>

### This consists of

<printlineEventStation>

interleave
<template>Any Text</template> optional
<filename>Any Text</filename> optional
</printlineEventStation>

### Places this can be found

In eventStation there is a choice between all of the following

- distanceRange
- printlineEventStation
- azimuthRange
- backAzimuthRange
- linearDistanceMagnitudeRange
- eventStationAND
- eventStationOR
- eventStationNOT
- midPoint
- removeStationDuplicate
- phaseExists
- phaseWithoutInterference
- eventStationScript
- externalEventStationSubsetter