### responseGain

Applies a overall sensitivity from the response to the seismograms, converting the digital counts into real world units. This is just a scalar multiplication factor, and hence no frequency dependency. To apply the response taking the frequency dependence of the response into account, use the processor. ResponseGain will convert int or short seismograms into floats to avoid rounding errors that could result in the output seismograms being all zeros. There is no configuration.

### Example

    <responseGain/>

### This consists of

<responseGain/>

### Places this can be found

In seismogramProcess there is a choice between all of the following

- printlineSeismogramProcess
- sacWriter
- mseedWriter
- asciiWriter
- wavWriter
- recordSectionDisplayGenerator
- responseGain
- phaseCut
- requestCut
- merge
- gapFill
- rMean
- rTrend
- taper
- externalWaveformProcess
- seismogramScript
- localSeismogramTemplateGenerator
- filter
- rms
- oregonDSPFilter
- forkProcess
- alwaysSuccess
- phaseSignalToNoise
- compoundPhaseSignalToNoise
- seismogramImageProcess
- legacyExecute
- seismogramAND
- seismogramOR
- seismogramNOT
- someDataCoverage
- noDataGaps
- fullDataCoverage
- integrate
- differentiate
- transferResponse
- collapseOverlaps
- div
- mul
- invertFlippedChannels
- seismogramSampling
- decimate
- stddev
- rms
- mean
- minMax
- compressionType
- availableDataPlus