### waveformVectorNOT

The output is the logical NOT of the output of the included waveformVector processors. This means that it will evaluate to true if the included processor evaluates to false, and vice versa. The seismic data passed down the chain is the data passed in. Seismogram results of the contained processors are ignored.

### Example

    <waveformVectorNOT>
        <rMean />
    </waveformVectorNOT>

### This consists of

<waveformVectorNOT>

waveformVectorProcessPlus choice
vectorAvailableDataPlus
waveformVectorProcess
</waveformVectorNOT>

### Places this can be found

In waveformVectorProcess there is a choice between all of the following

- threeComponentData
- ANDWaveformProcessWrapper
- ORWaveformProcessWrapper
- legacyVectorExecute
- waveformVectorFork
- waveformVectorAND
- waveformVectorOR
- waveformVectorNOT
- waveformVectorAlwaysSuccess
- seismogramProcess
- externalWaveformVectorProcess
- vectorImageProcess
- particleMotionPlot
- sampleSyncronize
- rotateGCP
- vectorTrim
- vectorScript
- iterDeconReceiverFunction